**Advanced Microcontroller Bus Architecture (AMBA) overview**

**What is Advanced Microcontroller Bus Architecture?**

AMBA is a standardized design MCU architecture which arm developed to simplify and standardize the design of microprocessors, microcontrollers, peripherals at very different levels of abstraction. It is made to be widely reused in different SoC parts and ASICs utilizing reusability, compatibility, flexibility and support.

Bus interfaces, like AMBA, in general are categorized according to their **Bandwidth & Latency**, therefore amba was made to try and achieve the best possible results in both fields.

AMBA has gradually developed over time, with different components/features being added to it to ensure it being a state-of-the-art architecture which something as impactful as Arm’s cortex M & several other influential and widely used paradigms to rely on.A screenshot of a computer

Description automatically generated

Figure 1: [AMBA versions, components & specifications](https://developer.arm.com/documentation/102202/0300/What-is-AMBA--and-why-use-it-)

***In this document we’re going to focus on AMBA AHB5, discuss its specifications & report on the design & verification***

**AMBA Advanced High-performance bus (AHB) lite overview**

A diagram of a machine

Description automatically generated

Figure 2  
 AMBA AHB lite

AMBA AHB is a bus interface suitable for   
**high-performance** synthesizable designs.   
It defines the interface between components,   
such as Managers, interconnects,   
and Subordinates.

AHB lite bus constituents:


* Managers
* Subordinates
* Address decoders
* Multiplexors

AMBA AHB implements the features required for high-performance, high clock frequency systems including:

* Burst transfers
* Single clock-edge operation
* Non-tristate implementation
* Configurable data bus widths
* Configurable address bus widths

The most common **AHB Subordinates** are internal memory devices, external memory interfaces, and high-bandwidth peripherals. Although low-bandwidth peripherals can be included as AHB Subordinates, for system performance reasons, they typically reside on the AMBA Advanced Peripheral Bus (APB). Bridging between the higher performance AHB and APB is done using an AHB Subordinate, known as an APB bridge.

**AMBA AHB lite Design components**

1. **Manager  
   A manager communicates with the subordinate through 2 types of feeds:**

* **Control Signals**
* **Data Signals**

**AHB also supports pipelined communication to increase throughput and maintain the high-performance paradigm.**

Figure 3   
AMBA AHB Manager

1. **Subordinate**

A diagram of a computer code

Description automatically generated**A subordinate receives transfers from the manager and responds accordingly:**

**The Subordinate signals back to the Manager:**

* **The completion or extension of the bus transfer.**
* **The success or failure of the bus transfer.**

Figure 4   
AMBA AHB Subordinate

1. **Interconnect**

**An interconnect component provides the connection between Managers and Subordinates in a system.**

**In case of Single Master-Multiple Subordinates (AHB lite), a decoder & a multiplexor are used in the interconnect’s stead.**

* **Decoder**The decoder receives the address provided by the Manager and in turn provides asserts the select line HSELx for the subordinate which the transaction is meant for.

The decoder also sends the same signal to the multiplexor delayed by the number of stages of the pipelining, or the number of cycles needed for the subordinate to provide a response.

A diagram of a decoder

Description automatically generatedA diagram of a network

Description automatically generatedA diagram of a computer code

Description automatically generated

Figure 5   
AMBA AHB lite decoder

The Manager side of the interconnect uses HTRANS to indicate valid transfers and has a single HREADY signal. HREADY is used to stall a transfer when the Subordinate has inserted wait states or when the Manager is waiting for arbitration from within the interconnect. The Subordinate side of the interconnect also includes an HSEL output and two HREADY signals. HREADYOUT from the Subordinate is passed to the Managers to insert wait states. The HREADY output from the interconnect can be used to stall a Subordinate if the data phase of the previoustransfer is stalled.  
  
An alternative implementation would be for HSEL to be tied HIGH on the Subordinates and the interconnect to override HTRANS to IDLE for unselected Subordinates.

Figure 7   
AMBA AHB Interconnect

* **Interconnect with AHB interfaces**Generic interconnect products can offer AHB as an interface option, among others such as AMBA AXI or AMBA APB. Figure 4-3 shows how a generic interconnect might implement HTRANS, HREADY, and HSEL.

Figure 6   
AMBA AHB lite Multiplexor

* **Multiplexor**The AHB protocol utilizes a read data multiplexor. After the Manager sends the address and control signals to all the Subordinates, with the decoder selecting the appropriate Subordinate during the data phase of the transfer. Any response data from the selected Subordinate, passes through the read data multiplexor to the Manager.

A diagram of a machine

Description automatically generated**Design of a re-configurable synthesizable pipelined AMBA AHB LITE**

Design constituents:

* Verification Environment acting as the Manager.
* Six Subordinates
* Address Decoder
* Multiplexor

Subordinate 1, 2 & 3:

* **Acting as normal subordinates** integrated with memory blocks (ROMs).
* Each requiring no privilege level from HPROT

Figure 8  
AMBA AHB lite depicting the connections between different subordinates & the manager

Re-Configurable Design:

* **HWDATA & HRDATA** data busses are reconfigurable to different widths **(32, 64, 128, 256, 512, 1024)** as per the specification document.
* **HADDR** address bus is reconfigurable to widths of **10 & 16 & 32** bits.

Subordinate 4:

* **Acting as the default subordinate** which is prescribed in the specifications document.
* Answering each select with an ERROR as well as a READY response.

Subordinate 5:

* **Acting as normal subordinates** integrated with memory blocks (ROMs).
* Requiring a specified privilege level from HPROT for WRITE operations.

Further Additions:

* For challenging verification dilemmas, I elected to **use ROMs instead of RAMs**.
* The data being transmitted is either opcode/data (not accounted for) while also being **non-cacheable and non-bufferable**.

Subordinate 6:

* **Acting as normal subordinates** integrated with memory blocks (ROMs).
* Requiring a specified privilege level from HPROT for WRITE & READ operations.


**AMBA AHB-lite test-plan**

|  |  |  |
| --- | --- | --- |
| TESTS | DESCRIPTION | NO. BUGS FOUND |
| 1. **reset\_test** | **:** Asserting reset for 15 clk cycles and checking the outputs | **Passed** |
| 1. **IDLE\_test** | **:** Randomizing stimulus and driving **HTRANS = IDLE** | **Passed** |
| 1. **WRITE\_SINGLE\_test** | **:** Randomizing stimulus and **READ** from the AHB subordinates **HBURST = SINGLE** | **Passed** |
| 1. **READ\_SINGLE\_test** | **:** Randomizing stimulus and **WRITE** to the AHB subordinates **HBURST = SINGLE** | **Passed** |
| 1. **WRITE\_INCR\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = INCR (randomized INCR length)** | **Passed** |
| 1. **READ\_INCR\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = INCR (randomized INCR length)** | **Passed** |
| 1. **WRITE\_READ\_INCR\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = INCR (randomized INCR length)** | **Passed** |
| 1. **WRITE\_WRAP4\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = WRAP4** | **Passed** |
| 1. **READ\_WRAP4\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = WRAP4** | **Passed** |
| 1. **WRITE\_READ\_WRAP4\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = WRAP4** | **Passed** |
| 1. **WRITE\_INCR4\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = INCR4** | **Passed** |
| 1. **READ\_INCR4\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = INCR4** | **Passed** |
| 1. **WRITE\_READ\_INCR4\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = INCR4** | **Passed** |
| 1. **WRITE\_WRAP8\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = WRAP8** | **Passed** |
| 1. **READ\_WRAP8\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = WRAP8** | **Passed** |
| 1. **WRITE\_READ\_WRAP8\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = WRAP8** | **Passed** |
| 1. **WRITE\_INCR8\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = INCR8** | **Passed** |
| 1. **READ\_INCR8\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = INCR8** | **Passed** |
| 1. **WRITE\_READ\_INCR8\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = INCR8** | **Passed** |
| 1. **WRITE\_WRAP16\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = WRAP16** | **Passed** |
| TESTS | DESCRIPTION | NO. BUGS FOUND |
| 1. **READ\_WRAP16\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = WRAP16** | **Passed** |
| 1. **WRITE\_READ\_WRAP16\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = WRAP16** | **Passed** |
| 1. **WRITE\_INCR16\_test** | **:** Randomizing stimulus and driving a **WRITE** with **HBURST = INCR16** | **Passed** |
| 1. **READ\_INCR16\_test** | **:** Randomizing stimulus and driving a **READ** with **HBURST = INCR16** | **Passed** |
| 1. **WRITE\_READ\_INCR16\_test** | **:** Randomizing stimulus and driving a **WRITE then READ** with **HBURST = INCR16** | **Passed** |
| 1. **ADDRESS\_ERROR\_INJECTION\_ test** | :Overriding constraints **to inject an invalid address during a burst transaction** **to check error response**. | **Passed** |
| 1. **PRIVILEGE\_ERROR\_INJECTION \_r\_test** | **: Overriding constraints to inject subordinate\_p\_r with a read operation without the correct HPROT value to check privilege error response** | **Passed** |
| 1. **PRIVILEGE\_ERROR\_INJECTION \_wr\_test** | **: Overriding constraints to inject subordinate\_p\_wr with a read & write operation without the correct HPROT value to check privilege error response** | **Passed** |
| 1. **runall\_test** |  |  |
| 1. **runall\_waited\_test** |  |  |

Coverage Groups

Instance based cover groups

* **HWDATA\_df\_cg: Covering the toggling of each bit of HWDATA*.***

**The next cover groups are made using an array of instances and are very applicable/easy to implement and use in functional toggling functional coverage**:  
HWDATA is a re-configurable bus that can be configured as low as 32 bits of width and up to 1024 bits of width. How can we ensure that all its driving pins/wires are working correctly without writing extensive & exhausting code? Through this.   
**HOW IT WORKS: Assume HWDATA is a 4-bit width bus**

Sample1 at 1st clock edge: HWDATA/vector = 0000 for example,

|  |  |  |  |
| --- | --- | --- | --- |
| i | position | vector | result |
| i = 0 | 0001 | 0000 | 0000 |
| i = 1 | 0010 | 0000 | 0000 |
| i = 2 | 0100 | 0000 | 0000 |
| i = 4 | 1000 | 0000 | 0000 |

**Now the bin of each instance has collected the coverage of ZERO for its respective bit of HWDATA.**   
Sample2 at 2nd clock edge: HWDATA/vector = 0101 for example,

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| I | position | vector | Initial result | result |
| i = 0 | 0001 | 0101 | 0000 | 0001 |
| i = 1 | 0010 | 0101 | 0000 | 0000 |
| i = 2 | 0100 | 0101 | 0000 | 0100 |
| i = 4 | 1000 | 0101 | 0000 | 0000 |

**Now the bin of each instance collects the coverage again, but this time, only 2 bits of HWDATA got toggled**


Sample3 at 3rd clock edge: HWDATA/vector = 1010 for example,

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| I | position | vector | Initial result | old result | result |
| i = 0 | 0001 | 1010 | 0000 | 0001 | 0000 |
| i = 1 | 0010 | 1010 | 0000 | 0000 | 0010 |
| i = 2 | 0100 | 1010 | 0000 | 0100 | 0000 |
| i = 4 | 1000 | 1010 | 0000 | 0000 | 1000 |

**Now the bin of each instance collects the coverage again, but this time, the remaining bits of HWDATA got toggled.**

**therefore achieving 100% coverage for toggling for wide buses.**

1. Making the cover group body:



1. Making the array of instances, an instance for each bit of the bus:



1. Construct each instance with the variable i being shifted to the left at each loop iteration (0001, 0010, 0100...etc.):



1. Sample each time the write function is called in the coverage collector:



**The previous cover** group covered the **toggling of data frame values of the bits of HWDATA bus**, **this one** covers the **toggling data transition values of the bits of HWDATA** bus.

* **HWDATA\_dt\_tog\_cg: Covering the toggling of each bit of HWDATA*.***

A close-up of a computer screen

AI-generated content may be incorrect.

**The next cover groups do the same for different busses**

* **HADDR\_df\_tog\_cg: Covering the toggling of each bit of HWDATA*.***
* **HADDR\_dt\_tog\_cg: Covering the toggling of each bit of HWDATA*.***
* **HSEL\_df\_tog\_cg: Covering the toggling of each bit of HWDATA*.***
* **HSEL\_dt\_tog\_cg: Covering the toggling of each bit of HWDATA*.***

A screenshot of a computer code

AI-generated content may be incorrect.

Coverage Groups (cont.)

Instance based cover groups

* **HSIZE\_dt\_cg: Covering the transitions of the HSIZE input values.**

This one is a bit tricky, since **HSIZE can take values up to 7, which in turn forces HWDATA & HRDATA to WRITE & READ up to 1024 bits of data (depending on the configuration), so for example, HSIZE being 7 while the bus is configured to bit width of 512 would ruin the functional coverage**, therefore, HSIZE’s array of instances width of the cover group is also controlled by the HWDATA\_WIDTH configuration.

1. Making the cover group body:

A computer code with colorful text

AI-generated content may be incorrect.

1. Making the array of instances for each possible value of HSIZE:



1. Construct each instance with the value of i being the predeterminant to all the possible values of HSIZE:



1. Sample each time the write function is called in the coverage collector:



**The previous cover** group covered the **data transition values of HTRANS**, **this one** covers the **data frame values of the of HTRANS** bus.

* **HTRANS\_df\_cg: Covering the toggling of each bit of HWDATA*.***

A computer screen shot of text

AI-generated content may be incorrect.

Coverage Groups (cont.)

Instance based cover groups

**The next cover groups do the same for each of the following buses, each having their own df & dt value cover points**

* **HRESET\_df\_cg: Covering the data frame of each value for HRESETn*.***
* **HTRANS\_df\_cg: Covering the data frame of each value for HTRANS*.***
* **HBURST\_df\_cg: Covering the data frame of each value for HBURST*.***
* **HSIZE\_df\_cg: Covering the data frame of each value for HSIZE**
* **HPROT\_df\_cg: Covering the data frame of each value for HPROT*.***

Traditional cover groups

* **RESET\_covgrp: Covering the changes & transition of HRESETn.**
* **WRITE\_covgrp: Covering the changes & transition of HWRITE.**
* **TRANS\_covgrp: Covering the changes & transition of HTRANS.**
* **BURST\_covgrp: Covering the changes & transition of HBURST.**
* **SIZE\_covgrp: Covering the changes & transitions of HSIZE.**
* **SUBORDINATE\_SELECT\_covgrp: Covering the changes & transitions of HSEL.**
* **ADDR\_covgrp: Covering the changes & transitions of HADDR.**
* **HWDATA\_covgrp: Covering the changes & transitions of the HWDATA with all its different SIZEs.**

**Creation of the cover groups**

A screen shot of a computer

AI-generated content may be incorrect.

**Sampling of the cover groups**

A blue square with white text

AI-generated content may be incorrect.

**Verification of a reconfigurable, pipelined AMBA AHB lite using UVM and SVA**


**Starting with the uvm hierarchy:**

**A screenshot of a computer

AI-generated content may be incorrect.**

**Issues faced during the verification process:**

* **Mimicking pipelining.**
* **Always blocks, counters & flag control**But then, using always blocks & control flags to mimic the behavior of pipelined stages seemed far maintainable, easier to use & debug. Also, much less of a hassle & different simulators have no hand in affecting the functionality due to different behaviors.
* **Reentrant tasks, events & fork-joins**At first, I thought about making a mix of reentrant functions, tasks and utilising fork - joins to mimic the pipelining of the design. Initially, it seemed to work, but it requires a lot of resources and is less reliable to debug & use. Also, different simulators behave differently with some of the elements used.

****

* **uvm\_tlm\_analysis\_fifo overwriting**
* **Always blocks, counters & flag control**But then, using always blocks & control flags to mimic the behavior of pipelined stages seemed far maintainable, easier to use & debug. Also, much less of a hassle & different simulators have no hand in affecting the functionality due to different behaviors.
* **Reentrant tasks, events & fork-joins**At first, I thought about making a mix of reentrant functions, tasks and utilising fork - joins to mimic the pipelining of the design. Initially, it seemed to work, but it requires a lot of resources and is less reliable to debug & use. Also, different simulators behave differently with some of the elements used.
  + A common misconception about how the class uvm\_tlm\_analysis\_fifo deals with **SCALAR variables vs. REFERENCE types**:
    - In Systemverilog **class objects & arrays** are almost always **passed by reference**, while **scalar variables** are always **passed by value**.
    - A diagram of a clock cycle

      Description automatically generatedTake **for example a pipelined design, a 3 stage pipelined design**, it takes **3 clock cycles for an input stimulus to be sent and for its output to progress through the DUT the output to be sampled**, in this scenario, one would have to write at least 3 times to the uvm\_tlm\_analaysis\_fifo (send 3 cycles of input stimulus to the inputs monitor then to the predictor and then the expected seq\_item is sent to the comparator P.S. both the predictor and the comparator are classes built in the scoreboard), and that is where the issue of overwriting occurs.

A blue rectangular object with white squares and black dots

Description automatically generated

**Issues faced during the verification process (cont.):**

* **uvm\_tlm\_analysis\_fifo overwriting (cont.)**

A diagram of a process

Description automatically generated

* + - In case of multiple writes using uvm\_tlm\_analysis\_fifo\_obj.write(seq\_item) to the uvm\_tlm\_analysis\_fifo without getting using the uvm\_tlm\_analysis\_fifo\_obj.get(seq\_item) after each write respectively. The uvm\_tlm\_analysis fifo does write indeed, and the functionality works correctly but the issue arises due to the fact that the .write function writes the handle to the memory location of the seq\_item, not the seq\_item itself, therefore if the handle of the seq\_item is not different on each write, the data that you’re trying to send over to the scoreboard will all be the same (same handle of the same seq\_item pointing to the same memory location).

**A diagram of a number of squares

Description automatically generated with medium confidence**

**Issues faced during the verification process (cont.):**

* **uvm\_tlm\_analysis\_fifo overwriting (cont.)**

**Solution?**

Create the seq\_item instance each time you write to the uvm\_tlm\_analysis\_fifo, that way, every instance handle is different inside the uvm\_tlm\_analysis\_fifo.

A diagram of a diagram

Description automatically generated

* **When is the test ending? Test Termination, How and When?**

At the start of the Verification process, the test was ending and therefore the scoreboard turning off before all the sequence items were processed and compared, which made me use the final\_phase to debug this behaviour.

A screenshot of a computer

AI-generated content may be incorrect.

To terminate the test only when all the items have been processed without complex logic in the interface & sequences, as well as remaining faithful to the uvm recommended practices & guidelines: I used 2 static unsigned integers (ints) comparator\_tr\_counter which increments after every comparison between an expected\_seq\_item & an actual\_seq\_item, as well as a predictor\_tr\_counter which increments after receiving an expected\_seq\_item in the comparator.

A screen shot of a computer

AI-generated content may be incorrect.

By using the phase\_ready\_to\_end phase and a task called delay\_phase, the scoreboard keeps a raised objection until both counters are equal to each other.


**P.S. The predictor\_tr\_counter is sometimes decremented during clearing the expected\_seq\_item\_fifo when an asynchronous reset is asserted**


**Issues faced during the verification process (cont.):**

* **Asynchronous reset in pipelined designs & verification environments**

When an Asynchronous reset is implemented, it means that basically when the reset is asserted, the entire design is reset at that same moment in time, which opens a very large number of possibilities of malfunctions for a verification engineer to take into consideration & cover. In a pipelined design, one of those malfunctions would be that if an Input is sent on X clk edge, it would take 3 more clock cycles for the output to progress through the DUT and to be sampled on X+3. Alternatively, in the verification environment, the stimulus that was sent on X clk edge, would be sent to the predictor class inside the scoreboard at time X as well, and therefore assessed accordingly, and the expected\_sequence\_item would be sent to the comparator and cannot be modified thereafter.

* **Proposed Solutions?**


****

****

****

After discussing with someone in the field the 3 solutions I came up with, I discovered that the clearing of the expected sequence fifo is the endorsed solution by most of the working engineers in the field.

**Issues faced during the verification process (cont.):  
Clearing the expected Sequence Item FIFO (Cont.)**But there is an issue that can occur with this solution, it is as demonstrated below:



As demonstrated above, **the reset is asserted when the past cycle was a write cycle**, The write transaction is sent to the predictor at the cycle before the reset, and the predictor acts accordingly (writes in the subordinate memory in the local subordinate ROM if it’s a write control/data command). On the other hand at the DUT, the address phase is sent, but the data phase is replaced by the reset, therefore preventing the write into the actual ROM of the DUT. **That is when my predictor runs a function to re-write the respective subordinate’s ROM location with the past value it had to avoid mismatch between the DUT’s ROM and the Predictor’s.**

P.S. This is why I implemented the design/verification environment with ROMs and not RAMs; to challenge myself to find a solution.

**Assertions REPORT**

|  |  |
| --- | --- |
| Feature | Assertion |
| The **reset assertion duration** should at least be **15 clock cycles**. | ***reset\_duration\_assert*** |
| **When reset is asserted,** no subordinates should be selected, i.e. **(HADDR = 0)** | **reset\_addr\_assert** |
| **When HTRANS == IDLE**, **HREADY** response should always be **HIGH** | **Idle\_ready\_assert** |
| **When HTRANS == IDLE**, inputs (HSIZE, HBURST, HWRITE) **should all be 0** | Idle\_inputs\_assert |
| **When a burst transfer** is issued, it must be followed by an **IDLE transfer** | **Incr4\_idle\_assert**  **Incr8\_idle\_assert**  **Incr16\_idle\_assert**  **wrap4\_idle\_assert**  **wrap8\_idle\_assert**  **wrap16\_idle\_assert** |
| **When a burst transfer** is issued, **HTRANS** must be == **NONSEQ** | **burst\_trans\_nonseq\_assert** |
| **When a burst transfer** is issued, **HTRANS** must be **== SEQ AFTER 1 CYCLE** (except for INCR burst) | **burst\_trans\_seq\_assert** |

**P.S. Check the coverage reports**.